A horse drawn carriage with text

Description automatically generated A qr code with black dots

Description automatically generated

**These instructions are a step by step guide on how to engage and disengage units with the safety stabilizing interlock system.**

**\*\*\*WE STRONGLY RECOMMEND CLICKING ON THE QR CODE ABOVE TO VIEW HOW-TO VIDEO\*\*\***

**Step 1** – Locate metal cap nut on the inside of drawer box at the back of drawer box

**Step 2** – To dis-engage - take index and middle finger and reach behind metal cap nut and locate cable behind drawer box

A black and white line

Description automatically generated

**Step 3** – Hook cable with both fingers (so the eye bolt is between them) and pull towards front of drawer box and move cable to the right and unhook from eye bolt.

A black and white drawing of a hand holding a nail

Description automatically generated A black and white line

Description automatically generated

**Step 4** – To re-engage – locate cable at back of cabinet and hook both fingers around cable and pull towards back of drawer box (front of cabinet) and hook onto eye bolt.

**For further assistance please contact Daniel’s Amish Collection at** [**info@danielsamish.com**](mailto:info@danielsamish.com) **or 330-276-0110**